From: ijackson@nyx.cs.du.edu (Ian Jackson)
Newsgroups: comp.os.linux.announce,comp.os.linux.answers,comp.os.linux.help,comp.os.linux.admin,comp.os.linux.misc,comp.os.linux.development,comp.answers,news.answers
Subject: Linux Frequently Asked Questions with Answers (FAQ: 1/2)
Date: Tue, 31 Jan 1995 23:48:09 GMT
Organization: Linux Unlimited
Message-ID: <ijackson-linux-faq2-0-1995@nyx.cs.du.edu>

Archive-Name: linux/faq/part1
Last-Modified: 31 Jan 1995

-----BEGIN PGP SIGNED MESSAGE-----

This is the list of Frequently Asked Questions about Linux, the free Unix
for 386/486/586 [see Q1.1 `What is Linux ?' for more details].  It should
be read in conjunction with the HOWTO documents, which are available in

* ftp.funet.fi (128.214.6.100) : /pub/OS/Linux/doc/HOWTO
* tsx-11.mit.edu (18.172.1.2) : /pub/linux/docs/HOWTO
* sunsite.unc.edu (152.2.22.81) : /pub/Linux/docs/HOWTO

and mirror sites thereof -- see Q2.5 `Where can I get Linux material by
FTP ?'.  See Q2.1 `Where can I get the HOWTOs and other documentation ?'
for a list of the HOWTOs and more information.  The INFO-SHEET and
META-FAQ, found in the same place, also list other sources of Linux
information.

The Linux Documentation Project documentation is available on
sunsite.unc.edu in /pub/Linux/docs/LDP.  These documents (more are in
preparation) are invaluable to the newcomer or for use as a reference
work.

Please check out these documents and this FAQ, especially Q12.1 `You still
haven't answered my question !', before posting your question to the
newsgroup comp.os.linux.help.

See Q13.2 `Formats in which this FAQ is available' for details of where to
get the PostScript, Emacs Info, HTML (WWW) and plain ASCII versions of
this document.

You can skip to a particular question by searching for `Question n.n'.

Note that this posting has been split into two parts because of its size.

A new version of this document appears approximately monthly.  If this
copy is more than a month old it may be out of date.

===============================================================================

Index

 Section 1.  Introduction and General Information
 Q1.1        What is Linux ?
 Q1.2        What software does it support ?
 Q1.3        Does it run on my computer ?  What hardware is supported ?
 Q1.4        What ports to other processors are there ?
 Q1.5        How much hard disk space does Linux need ?
 Q1.6        Is Linux PD ?  Copyrighted ?

 Section 2.  Network sources and resources
 Q2.1        Where can I get the HOWTOs and other documentation ?
 Q2.2        Where should I look on the World Wide Web for Linux stuff ?
 Q2.3        What newsgroups are there for Linux ?
 Q2.4        How do I install Linux ?
 Q2.5        Where can I get Linux material by FTP ?
 Q2.6        I don't have FTP access.  Where do I get Linux ?
 Q2.7        I don't have Usenet access.  Where do I get information ?
 Q2.8        What's this mailing list thing at niksula.hut.fi ?
 Q2.9        Are the newsgroups archived anywhere ?

 Section 3.  Compatibility with other operating systems
 Q3.1        Can Linux coexist with DOS ?  OS/2 ?  386BSD ?  Minix ?
 Q3.2        How do I access files on my DOS partition or floppy ?
 Q3.3        Can I use my Stacked/DBLSPC/etc. DOS drive ?
 Q3.4        Can I access OS/2 HPFS partitions from Linux ?
 Q3.5        Can I access BSD FFS, SysV UFS, Mac, Amiga, etc filesystems ?
 Q3.6        Can I run Microsoft Windows programs under Linux ?
 Q3.7        How can I boot Linux from OS/2's Boot Manager ?
 Q3.8        How can I share a swap partition between Linux and MS Windows ?

 Section 4.  Linux's handling of filesystems, disks and drives
 Q4.1        How can I undelete files ?
 Q4.2        Is there a defragmenter for ext2fs etc. ?
 Q4.3        How do I format and create a filesystem on a floppy ?
 Q4.4        I get nasty messages about inodes, blocks, and the suchlike
 Q4.5        My swap area isn't working.
 Q4.6        How do I remove LILO so my system boots DOS again ?
 Q4.7        Why can't I use fdformat except as root ?
 Q4.8        Is there something like Stacker or Doublespace for Linux ?
 Q4.9        My ext2fs partitions are checked each time I reboot.
 Q4.10       My root filesystem is read-only !
 Q4.11       I have a huge /proc/kcore !  Can I delete it ?
 Q4.12       My AHA1542C doesn't work with Linux.

 Section 5.  Porting, compiling and obtaining programs
 Q5.1        What is ld.so and where do I get it ?
 Q5.2        Has anyone ported / compiled / written XXX for Linux ?
 Q5.3        How do I port XXX to Linux ?
 Q5.4        Can I use code or a compiler compiled for a 486 on my 386 ?
 Q5.5        What does gcc -O6 do ?
 Q5.6        Where are <linux/*.h> and <asm/*.h> ?
 Q5.7        I get errors when I try to compile the kernel.
 Q5.8        How do I make a shared library ?
 Q5.9        How do I make my executables smaller ?
 Q5.10       Does Linux support threads or lightweight processes ?
 Q5.11       Where can I get `lint' for Linux ?

 Section 6.  Solutions to common miscellaneous problems
 Q6.1        Setuid scripts don't seem to work.
 Q6.2        Free memory as reported by free keeps shrinking.
 Q6.3        When I add more memory it slows to a crawl.
 Q6.4        Some programs (e.g. xdm) won't let me log in.
 Q6.5        Some programs let me log in with no password.
 Q6.6        My machine runs very slowly when I run GCC / X / ...
 Q6.7        I can only log in as root.
 Q6.8        My screen is all full of weird characters instead of letters.
 Q6.9        I have screwed up my system and can't log in to fix it.
 Q6.10       Emacs just dumps core.
 Q6.11       I've discovered a huge security hole in rm !
 Q6.12       lpr and/or lpd aren't working.
 Q6.13       Timestamps on files on msdos partitions are set incorrectly.

 Section 7.  How do I do this or find out that ... ?
 Q7.1        How can I get scrollback in text mode ?
 Q7.2        How do I switch virtual consoles ?  How do I enable them ?
 Q7.3        How do I set the timezone ?
 Q7.4        What version of Linux and what machine name am I using ?
 Q7.5        How can I enable or disable core dumps ?
 Q7.6        How do I upgrade/recompile my kernel ?
 Q7.7        Can I have more than 3 serial ports by sharing interrupts ?
 Q7.8        How do I make a bootable floppy ?
 Q7.9        How do I remap my keyboard to UK, French, etc. ?
 Q7.10       How do I get NUM LOCK to default to on ?
 Q7.11       How can I have more than 128Mb of swap ?

 Section 8.  Miscellaneous information and questions answered
 Q8.1        What is a .gz file ? And a .tgz ? And ... ?
 Q8.2        What does VFS stand for ?
 Q8.3        What is a BogoMip ?
 Q8.4        What is the Linux Journal and where can I get it ?
 Q8.5        How many people use Linux ?
 Q8.6        How should I pronounce Linux ?

 Section 9.  Frequently encountered error messages
 Q9.1        During linking I get Undefined symbol _mcount
 Q9.2        lp1 on fire
 Q9.3        INET: Warning: old style ioctl(IP_SET_DEV) called!
 Q9.4        ld: unrecognized option '-m486'
 Q9.5        GCC says Internal compiler error
 Q9.6        make says Error 139
 Q9.7        shell-init: permission denied when I log in.
 Q9.8        No utmp entry.  You must exec ... when I log in.
 Q9.9        Warning - bdflush not running
 Q9.10       Warning: obsolete routing request made.
 Q9.11       EXT2-fs: warning: mounting unchecked filesystem
 Q9.12       EXT2-fs warning: maximal count reached
 Q9.13       EXT2-fs warning: checktime reached
 Q9.14       df says Cannot read table of mounted filesystems
 Q9.15       fdisk says Partition X has different physical/logical ...
 Q9.16       fdisk: Partition 1 does not start on cylinder boundary
 Q9.17       fdisk says partition n has an odd number of sectors
 Q9.18       mtools says cannot initialise drive XYZ
 Q9.19       At the start of booting: Memory tight

 Section 10. The X Window System
 Q10.1       Does Linux support X Windows ?
 Q10.2       Where can I get an XF86Config for my system ?
 Q10.3       xterm logins show up strangely in who, finger
 Q10.4       I can't get X Windows to work right.

 Section 11. Questions applicable to very out-of-date software
 Q11.1       fdisk says cannot use nnn sectors of this partition
 Q11.2       GCC sometimes uses huge amounts of virtual memory and thrashes
 Q11.3       My keyboard goes all funny after I switch VC's.

 Section 12. How to get further assistance
 Q12.1       You still haven't answered my question !
 Q12.2       What to put in a posting to comp.os.linux.help
 Q12.3       I want to mail someone about my problem.

 Section 13. Administrative information and acknowledgements
 Q13.1       Feedback is invited
 Q13.2       Formats in which this FAQ is available
 Q13.3       Authorship and acknowledgements
 Q13.4       Disclaimer and Copyright

===============================================================================

Section 1.  Introduction and General Information

 Q1.1        What is Linux ?
 Q1.2        What software does it support ?
 Q1.3        Does it run on my computer ?  What hardware is supported ?
 Q1.4        What ports to other processors are there ?
 Q1.5        How much hard disk space does Linux need ?
 Q1.6        Is Linux PD ?  Copyrighted ?

- -----------------------------------------------------------------------------

Question 1.1.  What is Linux ?

Linux is a Unix clone written from scratch by Linus Torvalds with
assistance from a loosely-knit team of hackers across the Net.  It aims
towards POSIX compliance.

It has all the features you would expect in a modern fully-fledged Unix,
including true multitasking, virtual memory, shared libraries, demand
loading, shared copy-on-write executables, proper memory management and
TCP/IP networking.

It runs mainly on 386/486/586-based PCs, using the hardware facilities of
the 386 processor family (TSS segments et al) to implement these features.
Ports to other architectures are underway [Q1.4 `What ports to other
processors are there ?'].

See the Linux INFO-SHEET [Q2.1 `Where can I get the HOWTOs and other
documentation ?'] for more details.

The Linux kernel is distributed under the GNU General Public License - see
Q1.6 `Is Linux PD ?  Copyrighted ?' for more details.

- -----------------------------------------------------------------------------

Question 1.2.  What software does it support ?

Linux has GCC, Emacs, X-Windows, all the standard Unix utilities, TCP/IP
(including SLIP and PPP) and all the hundreds of programs that people have
compiled or ported for it.

There is a DOS emulator (look on tsx-11.mit.edu in
/pub/linux/ALPHA/dosemu) which can run DOS itself and some (but not all)
DOS applications.

An iBCS2 (Intel Binary Compatibility Standard) emulator for SVR4 ELF and
SVR3.2 COFF binaries is at a fairly advanced stage of development.  See
the iBCS2 emulator source tree README file for details.

Work is progressing on an emulator for Microsoft Windows binaries [Q3.6
`Can I run Microsoft Windows programs under Linux ?'].

For more information see the INFO-SHEET, which is one of the the HOWTOs
[Q2.1 `Where can I get the HOWTOs and other documentation ?'].  See also
Q5.3 `How do I port XXX to Linux ?'.

Some companies have commercial software available, including Motif.  They
announce their availability in comp.os.linux.announce --- try searching
the archives [Q2.9 `Are the newsgroups archived anywhere ?'].

- -----------------------------------------------------------------------------

Question 1.3.  Does it run on my computer ?  What hardware is supported ?

You need a 386, 486 or 586, with at least 2Mb of RAM and a single floppy,
to try it out.  To do anything useful more RAM and a hard disk are
required.

VESA local bus and PCI are both supported.  A driver for the NCR SCSI chip
in many PCI machines is included in current alpha test release kernels.

There are problems with machines using MCA (IBM's proprietary bus), mainly
to do with the hard disk controller.  There is a developers' release for
PS/2 ESDI drives on invaders.dcrl.nd.edu in /pub/misc/linux.  Certain
kinds of SCSI controllers also work, I understand.  Work is in progress to
create a suitable version of the Slackware distribution.  I'm afraid I
don't have any further details; you could try asking Arindam Banerji
<axb@defender.dcrl.nd.edu>.

Linux is reported to run on 386 family based laptops, with X on most of
them.

For details of exactly which PC's, video cards, disk controllers, etc.
work see the INFO-SHEET and the Hardware HOWTO [Q2.1 `Where can I get the
HOWTOs and other documentation ?'].

Linux will never run on a 286, because it uses task-switching and memory
management facilities only found on 386 family processors.

- -----------------------------------------------------------------------------

Question 1.4.  What ports to other processors are there ?

A project has been underway for a while to port Linux to suitable
68000-series based systems such as Amigas and Ataris.  This has now
reached beta test quality, but still lacks an X server.  There is a 680X0
channel on the Linux Activists mailserver [Q2.8 `What's this mailing list
thing at niksula.hut.fi ?'], and a Linux/68K FAQ on the World Wide Web and
on tsx-11.mit.edu in /pub/linux/680x0/FAQ.  There is a mailing list for
the Atari port - mail <majordomo@phil.uni-sb.de> with a body containing
only subscribe atarix - and an ftp area on ftp.phil.uni-sb.de in
/pub/atari/linux.

Information about a port to 68K-based Macintoshes can be found in the
MacLinux FAQ, available on www.ibg.uu.se in /pub/maclinux/FAQ.txt.  Other
stuff may be in the same directory.  There is a mailing list, but it is
currently broken.

Work has just been started on a port to the PowerPC.  Currently this will
be based on the PowerMAC architecture.  Again, don't post asking about it
unless you have experience to offer, and don't hold your breath.  There is
a mailing list - send your subscription request to
<linux-ppc-request@vger.rutgers.edu>.

On a political note, you might like to know that the FSF disapprove of
Apple - see /usr/lib/emacs/19.*/etc/APPLE on your system.

Both Linus and Jim Paradis <paradis@sousa.amt.ako.dec.com> or
<jrp@world.std.com> are working on ports to the 64-bit DEC AXP (the
Alpha).  Mailing list: <linux-alpha-request@vger.rutgers.edu>.

Ralf Baechle is working on a port to the MIPS, initially for the R4600 on
Deskstation Tyne machines.  The Linux/MIPS FAQ is available on the WWW and
in the MIPS port area on ftp.waldorf-gmbh.de in /pub/linux/mips.  There is
also a MIPS channel on the Linux Activists mailserver and a list
linux-mips at vger.rutgers.edu.  Interested people may mail their
questions and offers of assistance to <linux@waldorf-gmbh.de>.

None of these ports will be capable of running Linux/386 binaries.

- -----------------------------------------------------------------------------

Question 1.5.  How much hard disk space does Linux need ?

10Mb for a very minimal installation, suitable for trying it out and not
much else.

You can squeeze a more complete installation including X Windows into
80Mb.  Installating the whole of Slackware 1.2 takes around 200Mb,
including some space for user files and spool areas.

- -----------------------------------------------------------------------------

Question 1.6.  Is Linux PD ?  Copyrighted ?

The Linux kernel copyright belongs to Linus Torvalds.  He has placed it
under the GNU General Public Licence, which basically means that you may
freely copy, change and distribute it, but that you may not impose any
restrictions on further distribution, and that you must make the source
code available.  This is not the same as Public Domain (see the Copyright
FAQ, available on rtfm.mit.edu in
/pub/usenet/news.answers/law/Copyright-FAQ, for details).

Full details are in the file COPYING in the Linux kernel sources (probably
in /usr/src/linux on your system).

The licences of the utilities and programs which come with the
installations vary; much of the code is from the GNU Project at the Free
Software Foundation, and is also under the GPL.

Note that discussion about the merits or otherwise of the GPL should be
posted to gnu.misc.discuss and not to the comp.os.linux groups.

===============================================================================

Section 2.  Network sources and resources

 Q2.1        Where can I get the HOWTOs and other documentation ?
 Q2.2        Where should I look on the World Wide Web for Linux stuff ?
 Q2.3        What newsgroups are there for Linux ?
 Q2.4        How do I install Linux ?
 Q2.5        Where can I get Linux material by FTP ?
 Q2.6        I don't have FTP access.  Where do I get Linux ?
 Q2.7        I don't have Usenet access.  Where do I get information ?
 Q2.8        What's this mailing list thing at niksula.hut.fi ?
 Q2.9        Are the newsgroups archived anywhere ?

- -----------------------------------------------------------------------------

Question 2.1.  Where can I get the HOWTOs and other documentation ?

Look in the following places, and on sites that mirror them.

* ftp.funet.fi (128.214.6.100) : /pub/OS/Linux/doc/HOWTO
* tsx-11.mit.edu (18.172.1.2) : /pub/linux/docs/HOWTO
* sunsite.unc.edu (152.2.22.81) : /pub/Linux/docs/HOWTO

For a complete list of Linux FTP sites see Q2.5 `Where can I get Linux
material by FTP ?'.

If you don't have access to FTP try using the FTP-by-mail servers at
ftpmail@decwrl.dec.com, ftpmail@doc.ic.ac.uk or
ftp-mailer@informatik.tu-muenchen.de.

A complete list of HOWTO's is available in the file HOWTO.INDEX in the
docs/HOWTO directory at the FTP sites, but here is a (possibly incomplete)
list:

     Linux INFO-SHEET                        Linux META-FAQ
     BUPS HOWTO (regarding the Back UPS).    Busmouse HOWTO
     CDROM HOWTO                             Commercial HOWTO
     Distribution HOWTO                      DOSEMU HOWTO
     Ethernet HOWTO                          Ftape HOWTO
     German HOWTO                            Hardware HOWTO
     Installation HOWTO                      Japanese Extensions HOWTO
     Keystroke HOWTO                         Mail HOWTO
     MGR HOWTO                               NET-2 HOWTO
     NIS HOWTO (NIS is Sun's Yellow Pages)   News HOWTO
     PPP HOWTO                               Printing HOWTO
     SCSI HOWTO                              Sound HOWTO
     Term HOWTO                              Tips HOWTO
     UUCP HOWTO                              XFree86 HOWTO
More of these documents are always in preparation.  You should check in
nearby directories on the FTP sites if you can't find the answer in one of
the HOWTOs.  There are also a few mini-HOWTOs on sunsite.unc.edu in the
/pub/Linux/docs/HOWTO/mini directory.

The HOWTO.INDEX also contains information on how to write a new HOWTO.

The HOWTOs are coordinated by Matt Welsh, <mdw@sunsite.unc.edu>.

The `books' produced by the Linux Documentation Project are available in
/pub/Linux/docs/LDP on sunsite.unc.edu.  Please read them if you are new
to Unix and Linux.  Here is a list of those released so far:

* The Linux Documentation Project manifesto
* Installation and Getting Started Guide
* The Kernel Hacker's Guide
* Network Administration Guide
* Linux System Administrator's Guide

- -----------------------------------------------------------------------------

Question 2.2.  Where should I look on the World Wide Web for Linux stuff ?

Matt Welsh maintains the Linux Documentation Project Home Page, at
http://sunsite.unc.edu/mdw/linux.html.

This page refers to all the FAQs and HOWTOs, both those which are
available in HTML (WWW) format, like this FAQ, and those which aren't.

- -----------------------------------------------------------------------------

Question 2.3.  What newsgroups are there for Linux ?

There are five international Usenet newsgroups devoted to Linux.

comp.os.linux.announce is the moderated announcements group; you should
read this if you intend to use Linux.  Submissions for that group should
be emailed to linux-announce@tc.cornell.edu.

comp.os.linux.help, comp.os.linux.development, comp.os.linux.admin and
comp.os.linux.misc are also worth reading -- you may find that many common
problems are too recent to find in this FAQ but are answered in the
newsgroups.

Remember that since Linux is a Unix clone, most all of the material in
comp.unix.* and comp.windows.x.* groups will be relevant.  Apart from
hardware considerations, and some obscure or very technical low-level
issues, you'll find that these groups are the right place to start.

Please read Q12.1 `You still haven't answered my question !' before
posting, and make sure you post to the right newsgroup.  Crossposting is
rarely a good idea.

See also Q2.7 `I don't have Usenet access.  Where do I get information ?'.

Other regional and local newsgroups also exist - you may find the traffic
more manageable there.  The French Linux newsgroup is fr.comp.os.linux;
The German one is de.comp.os.linux.  In Australia, try
aus.computers.linux.

There may well be Linux groups local to your institution or area - check
there first.

- -----------------------------------------------------------------------------

Question 2.4.  How do I install Linux ?

There are several pre-packaged releases of Linux available, including the
MCC-Interim release, the TAMU release and the Slackware release.  Each
contains the software you need to run Linux, ready to install and use.
The exact details of which software is included and how to install them
vary from release to release.

You should read the Installation HOWTO for more details on how to go about
installing Slackware.  If you prefer a small, clean distribution to one
with everything but the kitchen sink you might like to try the MCC-Interim
release.

All of those releases are available via anonymous FTP from the Linux
archive sites [Q2.5 `Where can I get Linux material by FTP ?'].  There are
also a large number of other releases which are distributed less globally,
which suit special local and national requirements (for example, better
internationalisation support).

- -----------------------------------------------------------------------------

Question 2.5.  Where can I get Linux material by FTP ?

There are three main archive sites for Linux:

* ftp.funet.fi (Finland, 128.214.6.100) : /pub/OS/Linux
* sunsite.unc.edu (US, 152.2.22.81) : /pub/Linux
* tsx-11.mit.edu (US, 18.172.1.2) : /pub/linux

The MCC-Interim release is available from ftp.mcc.ac.uk (US, 130.88.200.7)
in /pub/linux; the TAMU release is available from net.tamu.edu (US,
128.194.177.1) in /pub/linux.

The contents of these sites is mirrored (copied, usually approximately
daily) by a number of other sites.  Please use one close to you -- that
will be faster for you and easier on the network.

* src.doc.ic.ac.uk : /packages/Linux (UK)
* sunacm.swan.ac.uk : /pub/Linux (UK)
* ftp.ibp.fr : /pub/linux (France)
* wuarchive.wustl.edu : /systems/linux (US)
* mrcnext.cso.uiuc.edu : /pub/linux (US)
* ftp.informatik.tu-muenchen.de : /pub/comp/os/linux (Germany)
* ftp.ibr.cs.tu-bs.de : /pub/os/linux (Germany)
* ftp.dfv.rwth-aachen.de : /pub/linux (Germany)
* ftp.informatik.rwth-aachen.de : /pub/Linux (Germany)
* bond.edu.au : /pub/OS/Linux (Australia)
* monu1.cc.monash.edu.au : /pub/linux (Australia)
* ftp.sun.ac.za : /pub/linux (South Africa)
* ftp.inf.utfsm.cl : /pub/Linux (Chile)

Not all of these mirror all of the other `source' sites, and some have
material not available on the `source' sites.

- -----------------------------------------------------------------------------

Question 2.6.  I don't have FTP access.  Where do I get Linux ?

The easiest thing is probably to find a friend with FTP access.  If there
is a Linux users group near you they may be able to help.

If you have a reasonably good email connection you could try the
FTP-by-mail servers at ftpmail@decwrl.dec.com, ftpmail@doc.ic.ac.uk or
ftp-mailer@informatik.tu-muenchen.de.

Linux is also available via traditional mail on diskette, CD-ROM and tape.
The Installation HOWTO, and the file /pub/Linux/docs/distributions on
sunsite.unc.edu, contain information on these distributions.

You could also try Zane Healy <healyzh@holonet.net>'s list of Linux BBS's,
which is posted regularly (1st and 15th of each month) to
comp.os.linux.announce and occasionally to the Fidonet and RIME UNIX
echoes.

- -----------------------------------------------------------------------------

Question 2.7.  I don't have Usenet access.  Where do I get information ?

Digests of postings to the comp.os.linux.* groups are available by
subscribing to the bidirectional gateway at
linux-*-request@news-digests.mit.edu, where * is one of announce,
development, help, misc or admin.

You are strongly advised to subscribe to at least
linux-announce-request@news-digests.mit.edu, as this carries important
information and documentation about Linux.

Please remember to use the -request addresses for your subscription and
unsubscription messages; mail to the other address is posted to the
newsgroup !

- -----------------------------------------------------------------------------

Question 2.8.  What's this mailing list thing at niksula.hut.fi ?

It's a multi-channel mailing list, mainly used by the developers of Linux
to talk about technical issues and future developments.  Most of the
channels are not intended for new users to ask their questions on.

Note that a new mailing list server is gaining rapid acceptance - send
message with list in the body to <majordomo@vger.rutgers.edu> (add help to
your mail if you don't have the standard Majordomo help file).  This
server contains lists corresponding to all of the channels at the niksula
multi-channel server (NB that these pairs of lists are *not* connected by
gateways - they are separate lists with the same target audience).

The ANNOUNCE list on niksula is a digest of postings to
comp.os.linux.announce, for the benefit of those without Usenet access.
However since niksula.hut.fi is slow and overloaded I'd recommend
subscribing to the MIT digestifier instead [Q2.7 `I don't have Usenet
access.  Where do I get information ?'].

There is also a NEWBIE channel (linux-newbie at vger) where `no question
is too stupid'; unfortunately it seems that few of the experienced users
read that channel, probably because of all the `stupid' questions !

If you want to subscribe to one or more of the channels at the niksula
multi-channel list, send an empty mail message to
linux-activists-request@niksula.hut.fi and you'll receive the instructions
for operating the list subscription software.

If you want to unsubscribe send a mail message like this
  From: you@domain.org
  To: linux-activists-request@niksula.hut.fi
  Subject: irrelevant

  X-Mn-Admin: leave CHANNEL
to leave a channel called CHANNEL.  Do *not* put an X-Mn-Key line in your
message - that will cause it to be posted to the list.

Note that you *must* remember to unsubscribe *before* you change your
email address, as due to a design flaw in the list server it is virtually
impossible to get yourself unsubscribed after such a change.

- -----------------------------------------------------------------------------

Question 2.9.  Are the newsgroups archived anywhere ?

Yes.  ftp.funet.fi and tsx-11.mit.edu contain archives of both
comp.os.linux.announce and the old group comp.os.linux, in their Linux
areas.  The comp.os.linux.announce archives are mirrored from /usenet on
src.doc.ic.ac.uk (which also contains another archive of comp.os.linux).

There is an `easy to access' archive of comp.os.linux.announce on the
World Wide Web at http://www.leo.org/archiv/linux/archiv/ann_index.html.
It supports searching and browsing.

===============================================================================

Section 3.  Compatibility with other operating systems

 Q3.1        Can Linux coexist with DOS ?  OS/2 ?  386BSD ?  Minix ?
 Q3.2        How do I access files on my DOS partition or floppy ?
 Q3.3        Can I use my Stacked/DBLSPC/etc. DOS drive ?
 Q3.4        Can I access OS/2 HPFS partitions from Linux ?
 Q3.5        Can I access BSD FFS, SysV UFS, Mac, Amiga, etc filesystems ?
 Q3.6        Can I run Microsoft Windows programs under Linux ?
 Q3.7        How can I boot Linux from OS/2's Boot Manager ?
 Q3.8        How can I share a swap partition between Linux and MS Windows ?

- -----------------------------------------------------------------------------

Question 3.1.  Can Linux coexist with DOS ?  OS/2 ?  386BSD ?  Minix ?

Yes.  Linux uses the standard PC partitioning scheme, so it can share your
disk with other operating systems.

Linux can read and write the files on your DOS and OS/2 FAT partitions and
floppies using either the DOS filesystem type built into the kernel or
mtools.  See Q1.2 `What software does it support ?' for details and status
of the emulators for DOS, MS Windows and System V programs.

Linux can also access Minix and System V UFS filesystems, and can read
(but not yet write) OS/2 HPFS and Amiga filesystems.

- -----------------------------------------------------------------------------

Question 3.2.  How do I access files on my DOS partition or floppy ?

Use the DOS filesystem, i.e. type, for example:
        mkdir /dos
        mount -t msdos -o conv=text,umask=022,uid=100,gid=100 /dev/hda3 /dos
If it's a floppy, don't forget to umount it before ejecting it !

You can use the conv=text/binary/auto, umask=nnn, uid=nnn and gid=nnn
options to control the automatic line-ending conversion, permissions and
ownerships of the files in the DOS filesystem as they appear under Linux.
If you mount your DOS filesystem by putting it in your /etc/fstab you can
record the options (comma-separated) there, instead of defaults.

Alternatively you can use `mtools', available in both binary and source
form on the FTP sites -- see Q2.5 `Where can I get Linux material by FTP
?'.

A kernel patch (known as the fd-patches) is available which allows
floppies with nonstandard numbers of tracks and/or sectors to be used;
this patch is included in the 1.1 alpha testing kernel series.

- -----------------------------------------------------------------------------

Question 3.3.  Can I use my Stacked/DBLSPC/etc. DOS drive ?

Not easily.  You can access them from within the DOS emulator [Q1.2 `What
software does it support ?'], but not as a normal filesystem under Linux
or using mtools.

- -----------------------------------------------------------------------------

Question 3.4.  Can I access OS/2 HPFS partitions from Linux ?

Yes, but it's only read-only at the moment.  To use it you must compile a
kernel with support for it enabled [Q7.6 `How do I upgrade/recompile my
kernel ?'].  Then you can mount it using the mount command, for example:
        mkdir /hpfs
        mount -t hpfs /dev/hda5 /hpfs

- -----------------------------------------------------------------------------

Question 3.5.  Can I access BSD FFS, SysV UFS, Mac, Amiga, etc filesystems ?

I'm told that there is a primitive, alpha test read-only Amiga filesystem
on sunsite.unc.edu in /pub/Linux/patches/amigaffs.tar.Z.  More information
is in affs-readme in the tarfile.

The 1.1.x alpha test kernel series contains support for the UFS filesystem
used by System V and Coherent.

There is a set of user-level programs that provides read-only access to
the Macintosh hierarchical filing system (HFS). It is available on
sunsite.unc.edu in /pub/Linux/utils/disk-management/xhfs0_3.tgz.

There is no support for the rest of those yet; I have not heard of any
recent work on providing some.

- -----------------------------------------------------------------------------

Question 3.6.  Can I run Microsoft Windows programs under Linux ?

Not yet.  There is a project, known as WINE, to build an MS Windows
emulator for Linux, but it is not ready for users yet.  Don't ask about it
unless you think you can contribute; look out for the status reports in
comp.emulators.ms-windows.wine.

In the meantime if you need to run MS Windows programs your best bet is
probably to reboot when you want to switch environments.  LILO (the Linux
bootloader) has the facility for a boot menu --- see its documentation for
more details.

- -----------------------------------------------------------------------------

Question 3.7.  How can I boot Linux from OS/2's Boot Manager ?

1. Create a partition using OS/2's FDISK (Not Linux's fdisk).

2. Format the partition under OS/2, either with FAT or HPFS.  This is so
that OS/2 knows about the partition being formatted.

3. Add the partition to the Boot Manager.

4. Boot Linux, and create a filesystem on the partition using mkfs -t ext2
or mke2fs.  At this point you may, if you like, use Linux's fdisk to
change the partition type code of the new partition to type 83 (Linux
Native) -- this may help some automated installation scripts find the
right partition to use.

5. Install Linux on the partition.

6. Install LILO on the Linux partition -- NOT on the master boot record of
the hard drive.  This installs LILO as a second-stage boot loader on the
Linux partition itself, to start up the kernel specified in the LILO
config file.  To do this you should put
   boot = /dev/hda2
(where /dev/hda2 is the *partition* you want to boot off) in your
/etc/lilo/config or /etc/lilo.config file.

7. Make sure that it is the Boot Manager partition that is marked active,
so that you can use Boot Manager to choose what to boot.

- -----------------------------------------------------------------------------

Question 3.8.  How can I share a swap partition between Linux and MS Windows ?

See the Mini-HOWTO on the subject by H. Peter Anvin, <hpa@eecs.nwu.edu>.
It is available on sunsite.unc.edu in /pub/Linux/docs.

===============================================================================

Section 4.  Linux's handling of filesystems, disks and drives

 Q4.1        How can I undelete files ?
 Q4.2        Is there a defragmenter for ext2fs etc. ?
 Q4.3        How do I format and create a filesystem on a floppy ?
 Q4.4        I get nasty messages about inodes, blocks, and the suchlike
 Q4.5        My swap area isn't working.
 Q4.6        How do I remove LILO so my system boots DOS again ?
 Q4.7        Why can't I use fdformat except as root ?
 Q4.8        Is there something like Stacker or Doublespace for Linux ?
 Q4.9        My ext2fs partitions are checked each time I reboot.
 Q4.10       My root filesystem is read-only !
 Q4.11       I have a huge /proc/kcore !  Can I delete it ?
 Q4.12       My AHA1542C doesn't work with Linux.

- -----------------------------------------------------------------------------

Question 4.1.  How can I undelete files ?

In general, this is very hard to do on Unices because of their
multitasking nature.  Undelete functionality for the ext2fs is being
worked on, but don't hold your breath.

There are a number of packages available that work by providing new
commands for deletion and sometimes copying that move deleted files into a
`wastebasket' directory instead; they can then be recovered until cleaned
out automatically by background processing.

Alternatively you can search the raw disk device which holds the
filesystem in question.  This is hard work, and you will need to be root
to do this.

- -----------------------------------------------------------------------------

Question 4.2.  Is there a defragmenter for ext2fs etc. ?

Yes.  There is a Linux filesystem defragmenter for minix, old-style, ext2,
and xia filesystems available on sunsite.unc.edu in
system/Filesystems/defrag-0.6.tar.gz.

Users of the ext2 filesystem can probably do without defrag since ext2
contains extra code to keep fragmentation reduced even in very full
filesystems.

- -----------------------------------------------------------------------------

Question 4.3.  How do I format and create a filesystem on a floppy ?

For a 3.5 inch high density floppy:
   fdformat /dev/fd0H1440
   mkfs -t ext2 -m 0 /dev/fd0H1440 1440
For a 5.25 inch floppy use fd0h1200 and 1200 as appropriate.  For the `B'
drive use fd1 instead of fd0.  Full details of which floppy devices do
what can be found in the Linux Device List [Q2.1 `Where can I get the
HOWTOs and other documentation ?'].  You may have to run mke2fs directly
instead of mkfs -t ext2.  The -m 0 option tells mkfs.ext2 not to reserve
any space on the disk for the superuser --- usually the last 10% is
reserved for root.

The first command low-level formats the floppy; the second creates an
empty filesystem on it.  After doing this you can mount the floppy like a
hard disk partition and simply cp and mv files, etc.

- -----------------------------------------------------------------------------

Question 4.4.  I get nasty messages about inodes, blocks, and the suchlike

You probably have a corrupted filesystem, probably caused by not shutting
Linux down properly before turning off the power or resetting.  You need
to use a recent shutdown program to do this --- for example, the one
included in the util-linux package, available on sunsite and tsx-11.

If you're lucky the program fsck (or e2fsck or xfsck as appropriate if you
don't have the automatic fsck front-end) will be able to repair your
filesystem; if you're unlucky the filesystem is trashed and you'll have to
reinitialise it with mkfs (or mke2fs, mkxfs etc.) it and restore from a
backup.

NB don't try to check a filesystem that's mounted read-write - this
includes the root partition if you don't see
   VFS: mounted root ... read-only
at boot time.

- -----------------------------------------------------------------------------

Question 4.5.  My swap area isn't working.

When you boot (or enable swapping manually) you should see
        Adding Swap: NNNNk swap-space

If you don't see any messages at all you are probably missing swapon -av
(the command to enable swapping) in your /etc/rc or /etc/rc.local (the
system startup scripts), or have forgotten to make the right entry in
/etc/fstab:
        /dev/hda2       none       swap       sw
for example.

If you see
        Unable to find swap-space signature
you have forgotten to run mkswap.  See the manpage for details; it works
much like mkfs.

Check the Installation HOWTO for detailed instructions of how to set up a
swap area.

- -----------------------------------------------------------------------------

Question 4.6.  How do I remove LILO so my system boots DOS again ?

Using DOS (MS-DOS 5.0 or later, or OS/2), type FDISK /MBR.  This will
restore a standard MS-DOS Master Boot Record.  If you have DR-DOS 6.0, go
into FDISK in the normal way and then select the `Re-write Master Boot
Record' option.

If you don't have DOS 5 or DR-DOS you need to have the boot sector that
LILO saved when you first installed it.  You did keep that file, didn't
you ?  It's probably called boot.0301 or some such.  Type
   dd if=boot.0301 of=/dev/hda bs=445 count=1
(or sda if you're using a SCSI disk).  This may also wipe out your
partition table, so beware !  If you're desperate, you could use
   dd if=/dev/zero of=/dev/hda bs=512 count=1
which will erase your partition table and boot sector completely: you can
then reformat the disk using your favourite software; however this will
render the contents of your disk inaccessible --- you'll lose it all
unless you're an expert.

Note that the DOS MBR boots whichever (single!) partition is flagged as
`active'; you may need to use fdisk to set and clear the active flags on
partitions appropriately.

- -----------------------------------------------------------------------------

Question 4.7.  Why can't I use fdformat except as root ?

The system call to format a floppy may only be done as root, regardless of
the permissions of /dev/fd0*.  If you want any user to be able to format a
floppy try getting the fdformat2 program; this works around the problems
by being setuid to root.

- -----------------------------------------------------------------------------

Question 4.8.  Is there something like Stacker or Doublespace for Linux ?

Currently none of the Linux filesystems can do compression in the
filesystem.

There is a transparently uncompressing C library, which is a drop-in
replacement for the standard C library.  It allows programs to read
compressed (ie, GNU zipped) files as if they were not compressed.  You
install it, and then you can compress files using gzip and have programs
still find them.  Look on sunsite.unc.edu in /pub/Linux/libs.  The author
is Alain Knaff <Alain.Knaff@imag.fr>.

There is a compressing block device driver that can provide
filesystem-independant on the fly disk compression in the kernel.  It is
called `DouBle'.  There is a source only distribution on sunsite.unc.edu
in /pub/Linux/utils/compress; the auther is Jean-Marc Verbavatz
<jmv@receptor.mgh.harvard.edu>.  Note that since this compresses inodes
(administrative information) and directories as well as file contents any
corruption is quite likely to be serious.

There is also a package available called tcx (Transparently Compressed
Executables) which allows you to keep infrequently used executables
compressed and only uncompress them temporarily while you use them.
You'll find it on the Linux FTP sites [Q2.5 `Where can I get Linux
material by FTP ?']; it was also announced in comp.os.linux.announce.
Note - this is not the same as gzexe, which is an inferior implementation
of the same concept.

- -----------------------------------------------------------------------------

Question 4.9.  My ext2fs partitions are checked each time I reboot.

See Q9.11 `EXT2-fs: warning: mounting unchecked filesystem'.

- -----------------------------------------------------------------------------

Question 4.10.  My root filesystem is read-only !

Remount it.  If /etc/fstab is correct you can simply mount -n -o remount
/. If /etc/fstab is wrong you must give the device name and posibly the
type too: e.g. mount -n -o remount -t ext2 /dev/hda2 /.  To understand why
you got into this state see Q9.11 `EXT2-fs: warning: mounting unchecked
filesystem'.

- -----------------------------------------------------------------------------

Question 4.11.  I have a huge /proc/kcore !  Can I delete it ?

None of the files in /proc are really there - they're all "pretend" files
made up by the kernel, to give you information about the system, and don't
take up any hard disk space.

/proc/kcore is like an "alias" for the memory in your computer; its size
is the same as the amount of RAM you have, and if you ask to read it as a
file the kernel does memory reads.

- -----------------------------------------------------------------------------

Question 4.12.  My AHA1542C doesn't work with Linux.

The option to allow disks with more than 1024 cylinders is only required
as a workaround for a DOS misfeature and should be turned *off* under
Linux.  For older Linux kernels you need to turn off most of the "advanced
BIOS" options - all but the one about scanning the bus for bootable
devices.

===============================================================================

Section 5.  Porting, compiling and obtaining programs

 Q5.1        What is ld.so and where do I get it ?
 Q5.2        Has anyone ported / compiled / written XXX for Linux ?
 Q5.3        How do I port XXX to Linux ?
 Q5.4        Can I use code or a compiler compiled for a 486 on my 386 ?
 Q5.5        What does gcc -O6 do ?
 Q5.6        Where are <linux/*.h> and <asm/*.h> ?
 Q5.7        I get errors when I try to compile the kernel.
 Q5.8        How do I make a shared library ?
 Q5.9        How do I make my executables smaller ?
 Q5.10       Does Linux support threads or lightweight processes ?
 Q5.11       Where can I get `lint' for Linux ?

- -----------------------------------------------------------------------------

Question 5.1.  What is ld.so and where do I get it ?

ld.so is the new dynamic library loader.  Each binary using shared
libraries used to have about 3K of start-up code to find and load the
shared libraries.  Now that code has been put in a special shared library,
/lib/ld.so, where all binaries can look for it, so that it wastes less
disk space, and can be upgraded more easily.

It can be obtained from tsx-11.mit.edu in /pub/linux/packages/GCC and
mirror sites thereof.  The latest version at the time of writing is
ld.so.1.4.4.tar.gz.

- -----------------------------------------------------------------------------

Question 5.2.  Has anyone ported / compiled / written XXX for Linux ?

First, look in the Linux Software Map (LSM) --- it's in the docs directory
on sunsite.unc.edu, and on the other FTP sties.

Check the FTP sites (see Q2.5 `Where can I get Linux material by FTP ?')
first --- search the find-ls or INDEX files for appropriate strings.
Check the Linux Projects Map (LPM), on ftp.ix.de in
/pub/Linux/docs/Projects-Map.gz.

If you don't find anything, you could either download the sources to the
program yourself and compile them -- see Q5.3 `How do I port XXX to Linux
?' -- or, if it's a large package which may require some porting, post a
message to the newsgroup.

If you compile a largeish program please upload it to one or more of the
FTP sites and post a message to comp.os.linux.announce (submit your
posting to <linux-announce@tc.cornell.edu>).

If you're looking for an application-type program the chances are someone
has already written a free verson.  Try reading the FAQ in
comp.sources.wanted for instructions on how to find sources.

You should also check the Projects-FAQ, available in
/pub/Linux/docs/faqs/Projects-FAQ on sunsite.unc.edu.

- -----------------------------------------------------------------------------

Question 5.3.  How do I port XXX to Linux ?

In general Unix programs need very little porting.  Simply follow the
installation instructions.  If you don't know and don't know how to find
out the answers to some of the questions asked during or by the
installation procedure you can guess, but this tends to produce buggy
programs.  In this case you're probably better off asking someone else to
do the port.

If you have a BSD-ish program you should try using -I/usr/include/bsd and
- -lbsd on the appropriate parts of the compilation lines.

- -----------------------------------------------------------------------------

Question 5.4.  Can I use code or a compiler compiled for a 486 on my 386 ?

Yes.

The -m486 option to GCC, which is used to compile binaries for 486
machines, merely changes certain optimisations.  This makes for slightly
larger binaries which run somewhat faster on a 486.  They still work fine
on a 386, though, with little performance hit.

GCC can be configured for a 386 or 486; the only difference is that
configuring it for a 386 makes -m386 the default and configuring for a 486
makes -m486 the default; in either case these can be overriden on a
per-compilation basis or by editing /usr/lib/gcc-lib/i*-linux/n.n.n/specs.

GCC does not currently know how to do optimisation well for the 586,
because Intel won't release the necessary information except under
nondisclosure.  Don't buy a Pentium or wait for people to reverse-engineer
the required optimisations.

- -----------------------------------------------------------------------------

Question 5.5.  What does gcc -O6 do ?

Currently the same as -O2; any number greater than 2 currently works just
like 2.  The Makefiles of newer kernels use -O2, and so should you.

GCC 2.6 adds optimisation level -O3.  However, GCC 2.6.0 and several of
the following versions are known to have some problems with Linux, though
these will hopefully be solved soon.  In any case you should not use -O3
on a program until you're sure it doesn't create any problems.

- -----------------------------------------------------------------------------

Question 5.6.  Where are <linux/*.h> and <asm/*.h> ?

These are in the directories /usr/include/linux and /usr/include/asm.

However they should be symbolic links to your kernel sources in
/usr/src/linux and not real directories.

If you don't have the kernel sources download them --- see Q7.6 `How do I
upgrade/recompile my kernel ?'.

Then use rm to remove any garbage, and ln to create the links:
   rm -rf /usr/include/linux /usr/include/asm
   ln -sf /usr/src/linux/include/linux /usr/include/linux
   ln -sf /usr/src/linux/include/asm /usr/include/asm

- -----------------------------------------------------------------------------

Question 5.7.  I get errors when I try to compile the kernel.

Make sure that /usr/include/linux and /usr/include/asm aren't actual
directories but instead symbolic links to /usr/src/linux/include/linux and
/usr/src/linux/include/asm respectively.

If necessary, delete them using rm and then use ln -s to make the links as
in Q5.6 `Where are <linux/*.h> and <asm/*.h> ?'.

Remember that when you apply a patch to the kernel you must use the -p0 or
- -p1 option: otherwise the patch may be misapplied.  See the manpage for
patch for details.

If you're using a kernel more recent than 1.1.44 you should find that
there are new directories /usr/src/linux/include/asm-i386.  The directory
asm there should be removed, as should the directory asm.  The symlinks
Makefile target will make these be symbolic links to asm-i36 and
arch/i386/boot respectively.  The easiest way to make sure all this gets
done is not to try to patch 1.1.44 to make 1.1.45, but to download
linux-1.1.45.tar.gz instead.

ld: unrecognised option `-qmagic' means you should get a newer linker,
from tsx-11.mit.edu in /pub/linux/packages/GCC, in the file
image-4.6.xx.tar.gz.

- -----------------------------------------------------------------------------

Question 5.8.  How do I make a shared library ?

Get tools-n.nn.tar.gz from tsx-11.mit.edu, in /pub/linux/packages/GCC/src.
It comes with documentation that will tell you what to do.

- -----------------------------------------------------------------------------

Question 5.9.  How do I make my executables smaller ?

The most common cause of large executables is the -g compiler flag.  This
produces (as well as debugging information in the output file) a program
which is statically linked, i.e. one which includes a copy of the C
library instead of using a dynamically linked copy.

Other things that are worth investigating are -O and -O2 which enable
optimisation (check the GCC documentation) and -s which strips the symbol
information from the resulting binary (making debugging totally
impossible).

You may wish to use -N on very small executables (less than 8K with the
- -N), but you shouldn't do this unless you understand its performance
implications, and definitely never with daemons.

Using QMAGIC binaries also can reduce the size of binaries, especially
small ones.  Don't worry about this unless you know what QMAGIC is; Linux
is moving to QMAGIC as a default.

- -----------------------------------------------------------------------------

Question 5.10.  Does Linux support threads or lightweight processes ?

As well as the Unix multiprocessing model involving heavyweight processes,
which is of course part of the standard Linux kernel, there are several
implementations of lightweight processes or threads, most of which are
generic packages for any Unix:

* In sipb.mit.edu:/pub/pthread or ftp.ibp.fr:/pub/unix/threads/pthreads.
  Documentation isn't in the package, but is available on the World Wide
  Web at http://www.mit.edu:8001/people/proven/home_page.html.
* In ftp.cs.washington.edu:/pub/qt-001.tar.Z is QuickThreads.  More
  information can be found in the technical report, available on the same
  site as /tr/1993/05/UW-CSE-93-05-06.PS.Z.
* In gummo.doc.ic.ac.uk:/rex is lwp, a very minimal implementation.
* In ftp.cs.fsu.edu:/pub/PART, an Ada implementation.  This is useful
  mainly because it has a lot of PostScript papers that you'll find useful
  in learning more about threads.  This is not directly useable under
  Linux.

Please contact the authors of the packages in question for details.

- -----------------------------------------------------------------------------

Question 5.11.  Where can I get `lint' for Linux ?

Roughly equivalent functionality is built into the GNU C compiler (gcc)
which is used by Linux systems.  Use the -Wall option to turn on most of
the useful extra warnings.  Check the GCC manual for more details (type
control-h followed by i in Emacs and select the entry for GCC).

===============================================================================

The remainder of the FAQ is in the next part ...


-----BEGIN PGP SIGNATURE-----
Version: 2.6

iQCVAgUBLy7NbsMWjroj9a3bAQHq8gP+PuZKirYlRw2gA4PIqsRGQO5qomf16WOU
MNGsFjwpX1/I2YMzlldeFNEgAZ37J7whwBI+RtYlRJh+DA8XC8dDjeGPYo9Kl7O6
AeOCRPmqu/vFtnFGS+Ni2MRJySMz7IXiP/lLBLfKff2s9mOPTFVJQeu0yGL9e11e
6syif97kZN8=
=87kG
-----END PGP SIGNATURE-----
-- 
Ian Jackson, at home.         ijackson@nyx.cs.du.edu or iwj10@cus.cam.ac.uk
+44 1223 575512    Escoerea on IRC.   http://www.cl.cam.ac.uk/users/iwj10/
2 Lexington Close, Cambridge, CB4 3LS, England.   Urgent: iwj@cam-orl.co.uk

From: ijackson@nyx.cs.du.edu (Ian Jackson)
Newsgroups: comp.os.linux.announce,comp.os.linux.answers,comp.os.linux.help,comp.os.linux.admin,comp.os.linux.misc,comp.os.linux.development,comp.answers,news.answers
Subject: Linux Frequently Asked Questions with Answers (FAQ: 2/2)
Date: Tue, 31 Jan 1995 23:49:04 GMT
Organization: Linux Unlimited
Message-ID: <ijackson-linux-faq2-0-1995-pt2@nyx.cs.du.edu>

Archive-Name: linux/faq/part2
Last-Modified: 31 Jan 1995

-----BEGIN PGP SIGNED MESSAGE-----

(Continued from part 1, where you'll find the introduction and
 table of contents.)
===============================================================================

Section 6.  Solutions to common miscellaneous problems

 Q6.1        Setuid scripts don't seem to work.
 Q6.2        Free memory as reported by free keeps shrinking.
 Q6.3        When I add more memory it slows to a crawl.
 Q6.4        Some programs (e.g. xdm) won't let me log in.
 Q6.5        Some programs let me log in with no password.
 Q6.6        My machine runs very slowly when I run GCC / X / ...
 Q6.7        I can only log in as root.
 Q6.8        My screen is all full of weird characters instead of letters.
 Q6.9        I have screwed up my system and can't log in to fix it.
 Q6.10       Emacs just dumps core.
 Q6.11       I've discovered a huge security hole in rm !
 Q6.12       lpr and/or lpd aren't working.
 Q6.13       Timestamps on files on msdos partitions are set incorrectly.

- -----------------------------------------------------------------------------

Question 6.1.  Setuid scripts don't seem to work.

That's right.  This feature has been deliberately disabled in the Linux
kernel because setuid scripts are almost always a security hole.  If you
want to know why read the FAQ for comp.unix.questions.

- -----------------------------------------------------------------------------

Question 6.2.  Free memory as reported by free keeps shrinking.

The `free' figure printed by free doesn't include memory used as a disk
buffer cache - shown in the `buffers' column.  If you want to know how
much memory is really free add the `buffers' amount to `free'.

The disk buffer cache tends to grow soon after starting Linux up, as you
load more programs and use more files and the contents get cached.  It
will stabilise after a while.

- -----------------------------------------------------------------------------

Question 6.3.  When I add more memory it slows to a crawl.

This is quite a common symptom of a failure to cache the additional
memory.  The exact problem depends on your motherboard.

Sometimes you have to enable caching of certain regions in your BIOS
setup.  Look in the CMOS setup and see if there is an option to cache the
new memory area which is currently switched off.  This is apparently most
common on a 486.

Sometimes the RAMs have to be in certain sockets to be cached.

Sometimes you have to set jumpers to enable the caching.

Some motherboards don't cache all the RAM if you have more RAM per amount
of cache than they expect.  Usually a full 256K cache will solve this
problem.

If in doubt, check your motherboard manual.  If you still can't fix it
because the documentation is inadequate you might like to post a message
giving *all* the details - make, model number, date code, etc. so that
other Linux users can avoid it.

- -----------------------------------------------------------------------------

Question 6.4.  Some programs (e.g. xdm) won't let me log in.

You are probably using non-shadow-password programs but are using shadow
passwords.

If so, you have to get or compile a shadow password version of the
program(s) in question.  The shadow password suite can be found in
(amongst other places):
   tsx-11.mit.edu:/pub/linux/sources/usr.bin/shadow-*
This is the source code; you will probably find the binaries in
.../linux/binaries/usr.bin.

- -----------------------------------------------------------------------------

Question 6.5.  Some programs let me log in with no password.

You probably have the same problem as in Q6.4 `Some programs (e.g. xdm)
won't let me log in.', with an added wrinkle:

If you are using shadow passords you should put an asterisk in the
password field of /etc/passwd for each account, so that if a program
doesn't know about the shadow passwords it won't think it's a passwordless
account and let anyone in.

- -----------------------------------------------------------------------------

Question 6.6.  My machine runs very slowly when I run GCC / X / ...

You may not have any swap enabled.  You need to enable swapping to allow
Linux to page out bits of data programs aren't using at the moment to disk
to make more room for other programs and data.  If you don't Linux has to
keep data in memory and throw away in-memory copies of programs (which are
paged straight from the filesystem) and so less and less program is in
memory and everything runs very slowly.

See the Installation HOWTO and the Installation and Getting Started Guide
[Q2.1 `Where can I get the HOWTOs and other documentation ?'] for details
of how to set up a swap partition or swapfile; see also Q4.5 `My swap area
isn't working.'.

Alternatively you may have too little real memory.  If you have less RAM
than all the programs you're running at once use Linux will use your hard
disk instead and thrash horribly.  The solution in this case is to not run
so many things at once or to buy more memory.  You can also reclaim some
memory by compiling and using a kernel with less options configured.  See
Q7.6 `How do I upgrade/recompile my kernel ?'.

You can tell how much memory and/or swap you're using by using the free
command, or by typing
    cat /proc/meminfo

If your kernel is configured with a ramdisk this is probably wasted space
and will cause things to go slowly.  Use LILO or rdev to tell the kernel
not to allocate a ramdisk (see the LILO documentation or type man rdev).

- -----------------------------------------------------------------------------

Question 6.7.  I can only log in as root.

You probably have some permission problems, or you have a file
/etc/nologin.

If the latter put rm -f /etc/nologin in your /etc/rc or /etc/rc.local.

Otherwise check the permissions on your shell, and any filenames which
appear in error messages, and also the directories containing these files
all the way back up the tree to the root directory.

- -----------------------------------------------------------------------------

Question 6.8.  My screen is all full of weird characters instead of letters.

You probably sent some binary data to your screen by mistake.  Type echo
^V^[c (that's e c h o space control-V escape c return) to fix it.  Many
Linux distributions have a command reset that does this.

- -----------------------------------------------------------------------------

Question 6.9.  I have screwed up my system and can't log in to fix it.

Reboot from an emergency floppy or floppy pair, for example the Slackware
boot- and root-disk pair (in the install subdirectory of the Slackware
mirrors) or the MCC installation boot floppy.  There are also two diy
rescue disk creation packages on sunsite.unc.edu in
/pub/Linux/system/Recovery.  These are better as they'll have your own
kernel on them, so that you don't run the risk of missing devices,
filesystems, etc.

Get to a shell prompt and mount your hard disk with something like
   mount -t ext2 /dev/hda1 /mnt

Then your filesystem is available under the directory /mnt and you can fix
the problem.  Remember to unmount your hard disk before rebooting (cd back
down to / first or it will say it's busy).

- -----------------------------------------------------------------------------

Question 6.10.  Emacs just dumps core.

You probably have the X version of Emacs that comes with SLS.  It doesn't
work without the X libraries.  The solution is to install X Windows or get
a newer Emacs binary without any X Windows support.

- -----------------------------------------------------------------------------

Question 6.11.  I've discovered a huge security hole in rm !

No you haven't.  You are obviously new to Unix and need to read a good
book on it to find out how things work.  Clue: ability to delete files
under Unix depends on permission to write the directory they are in.

- -----------------------------------------------------------------------------

Question 6.12.  lpr and/or lpd aren't working.

Check the Printing HOWTO [Q2.1 `Where can I get the HOWTOs and other
documentation ?'].

- -----------------------------------------------------------------------------

Question 6.13.  Timestamps on files on msdos partitions are set incorrectly.

There is a bug in the program clock (often found in /sbin) - it miscounts
a timezone offset, confusing seconds with minutes or some such.  Get a new
version of it.

===============================================================================

Section 7.  How do I do this or find out that ... ?

 Q7.1        How can I get scrollback in text mode ?
 Q7.2        How do I switch virtual consoles ?  How do I enable them ?
 Q7.3        How do I set the timezone ?
 Q7.4        What version of Linux and what machine name am I using ?
 Q7.5        How can I enable or disable core dumps ?
 Q7.6        How do I upgrade/recompile my kernel ?
 Q7.7        Can I have more than 3 serial ports by sharing interrupts ?
 Q7.8        How do I make a bootable floppy ?
 Q7.9        How do I remap my keyboard to UK, French, etc. ?
 Q7.10       How do I get NUM LOCK to default to on ?
 Q7.11       How can I have more than 128Mb of swap ?

- -----------------------------------------------------------------------------

Question 7.1.  How can I get scrollback in text mode ?

With the default US keymap you can use Shift with the PageUp and PageDown
keys (NB these must be the grey ones, not the ones on the numeric keypad
!).  With other keymaps check the maps in /usr/lib/keytables; you can
remap the scroll up and down keys to be whatever you like --- for example,
in order to remap them to keys that exist on an 84-key AT keyboard.

You can't increase the amount of scrollback, because of the way it is
implemented using the video memory to store the scrollback text, though
you may be able to get more scrollback in each virtual console by reducing
the total number of VC's --- see <linux/tty.h>.

- -----------------------------------------------------------------------------

Question 7.2.  How do I switch virtual consoles ?  How do I enable them ?

In text mode, press (Left) Alt-F1 to Alt-F12 to select the consoles tty1
to tty12.  To switch out of X windows you must press Ctrl-Alt-F1 etc;
Alt-F5 or whatever will switch back.

Your kernel probably doesn't have all 12 compiled in; the default is 8.
This is controlled by NR_CONSOLES in linux/include/linux/tty.h.

If you want to use a VC for ordinary login you need to list it in
/etc/inittab, which controls which terminals and virtual consoles have
login prompts.  NB: X needs at least one free VC in order to start.

- -----------------------------------------------------------------------------

Question 7.3.  How do I set the timezone ?

Change directory to /usr/lib/zoneinfo; get the timezone package if you
don't have this directory.  The source can be found on sunsite.unc.edu in
/pub/Linux/system/Admin/timesrc-1.2.tar.gz.

Then make a symbolic link named localtime pointing to one of the files in
this directory (or a subdirectory), and one called posixrules pointing to
localtime.  For example:
   ln -sf US/Mountain localtime
   ln -sf localtime posixrules
This change will take effect immediately - try date.

Don't try to use the TZ variable - leave it unset.

You should also make sure that your Linux kernel clock is set to the
correct GMT time - type date -u and check that the correct universal time
is displayed.

- -----------------------------------------------------------------------------

Question 7.4.  What version of Linux and what machine name am I using ?

Type:
   uname -a

- -----------------------------------------------------------------------------

Question 7.5.  How can I enable or disable core dumps ?

Since 0.99pl14 Linux has had corefiles turned off by default for all
processes.

You can turn them on or off by using the ulimit command in bash, or the
limit command in tcsh.  See the manpage for the shell for more details.

That command affects all programs run from that shell (directly or
indirectly), not the whole system.

If you wish to enable or disable coredumping for all processes by default
you can change the default setting in <linux/sched.h> - see the definition
of INIT_TASK.

- -----------------------------------------------------------------------------

Question 7.6.  How do I upgrade/recompile my kernel ?

See the README which comes with the kernel release on ftp.funet.fi, in
/pub/OS/Linux/PEOPLE/Linus and mirrors thereof.  Try to get it from a
closer site if possible; ftp.funet.fi is a very busy site and therefore
slow -- see Q2.5 `Where can I get Linux material by FTP ?'.  You may
already have a version of the kernel source code installed on your system,
but if you got it as part of a standard distribution it is likely to be
somewhat out of date (this is not a problem if you only want a
custom-configured kernel, but it probably is if you need to upgrade.)

Remember that to make the new kernel boot you must run LILO after copying
the kernel into your root partition -- the Makefile in recent kernels has
a special zlilo target for this; try make zlilo.

Russel Nelson posts summaries of what changes in recent kernel patches to
comp.os.linux.development, and these are archived on ftp.emlist.com in
/pub/kchanges.

- -----------------------------------------------------------------------------

Question 7.7.  Can I have more than 3 serial ports by sharing interrupts ?

Not without some trickery.  This is a limitation of the ISA bus
architecture.

See the Serial HOWTO for information about how to work around this
problem.

- -----------------------------------------------------------------------------

Question 7.8.  How do I make a bootable floppy ?

Make a filesystem on it with bin, etc and lib directories -- everything
you need.  Install a kernel on it and arrange to have LILO boot it from
the floppy (see the LILO documentation, in lilo.u.*.ps).

If you build the kernel (or tell LILO to tell the kernel) to have a
ramdisk the same size as the floppy the ramdisk will be loaded at
boot-time and mounted as root in place of the floppy.

- -----------------------------------------------------------------------------

Question 7.9.  How do I remap my keyboard to UK, French, etc. ?

For recent kernels, get kbd*.tar.gz from the same place as you got the
kernel source.  Make sure you get the appropriate version; you have to use
the right keyboard-mapping package to go with your kernel version.  The
latest at the time of writing is kbd-0.85.tar.gz, which works with kernel
versions from 1.0.

For older kernels you have to edit the top-level kernel Makefile, in
/usr/src/linux.

You may find more helpful information in the Keystroke HOWTO, on
sunsite.unc.edu in /pub/Linux/docs/HOWTO/Keystroke-HOWTO.

- -----------------------------------------------------------------------------

Question 7.10.  How do I get NUM LOCK to default to on ?

Use the setleds program, for example (in /etc/rc.local):
   for t in 1 2 3 4 5 6 7 8
   do
        setleds +num < /dev/tty$t > /dev/null
   done

setleds is part of the kbd-0.8x package (see Q7.9 `How do I remap my
keyboard to UK, French, etc. ?').

Alternatively, patch your kernel.  You need to arrange for KBD_DEFLEDS to
be defined to (1 << VC_NUMLOCK) when compiling drivers/char/keyboard.c.

- -----------------------------------------------------------------------------

Question 7.11.  How can I have more than 128Mb of swap ?

Use several swap partitions or swapfiles - Linux supports up to 16 swap
areas, each of up to 128Mb.

Very old kernels only supported swap area sizes up to 16Mb.

===============================================================================

Section 8.  Miscellaneous information and questions answered

 Q8.1        What is a .gz file ? And a .tgz ? And ... ?
 Q8.2        What does VFS stand for ?
 Q8.3        What is a BogoMip ?
 Q8.4        What is the Linux Journal and where can I get it ?
 Q8.5        How many people use Linux ?
 Q8.6        How should I pronounce Linux ?

- -----------------------------------------------------------------------------

Question 8.1.  What is a .gz file ? And a .tgz ? And ... ?

.gz (and .z) files have been compressed using GNU gzip.  You need to use
gunzip (which is as a symlink to the gzip command which comes with most
Linux installations) to unpack the file.

.taz and .tz are tarfiles (made with Unix tar) compressed using standard
Unix compress.

.tgz (or .tpz) is a tarfile compressed with gzip.

.lsm is a Linux Software Map entry, in the form of a short text file.
Details about the LSM and the LSM itself are available in the docs
subdirectory on sunsite.unc.edu.

The file command can often tell you what a file is.

If you find that gzip complains when you try to uncompress a gzipped file
you probably downloaded it in ASCII mode by mistake.  You must download
most things in binary mode - remember to type binary as a command in FTP
before using get to get the file.

- -----------------------------------------------------------------------------

Question 8.2.  What does VFS stand for ?

Virtual File System.  It's the abstraction layer between the user and real
filesystems like ext2, minix and msdos.  Amongst other things, its job is
to flush the read buffer when it detects a disk change on the floppy disk
drive:
   VFS: Disk change detected on device 2/0

- -----------------------------------------------------------------------------

Question 8.3.  What is a BogoMip ?

`BogoMips' is a contraction of `Bogus MIPS'.  MIPS stands for (depending
who you listen to) Millions of Instructions per Second, or Meaningless
Indication of Processor Speed.

The number printed at boot-time is the result of a kernel timing
calibration, used for very short delay loops by some device drivers.

As a very rough guide the BogoMips will be approximately:
     386SX              clock * 0.14
     386DX              clock * 0.18
     486Cyrix/IBM       clock * 0.33
     486SX/DX/DX2       clock * 0.50
     586                clock * 0.39

If the number you're seeing is wildly lower than this you may have the
Turbo button or CPU speed set incorrectly, or have some kind of caching
problem [as described in Q6.3 `When I add more memory it slows to a
crawl.'.]

For values people have seen with other, rarer, chips, see the BogoMips
Mini-HOWTO, on sunsite.unc.edu in /pub/Linux/docs/howto/mini/BogoMips.

- -----------------------------------------------------------------------------

Question 8.4.  What is the Linux Journal and where can I get it ?

Linux Journal is a monthly magazine (printed on paper) that is available
on newsstands and via subscription worldwide. Email <linux@ssc.com> for
details.

- -----------------------------------------------------------------------------

Question 8.5.  How many people use Linux ?

Linux is freely available, and no one is required to register their copies
with any central authority, so it is difficult to know.  Several
businesses are now surviving solely on selling and supporting Linux, and
very few Linux users use those businesses, relatively speaking.  The Linux
newsgroups are some of the most heavily read on the Net, so the number is
likely in the hundreds of thousands, but firm numbers are hard to come by.

However, one brave soul, Harald T. Alvestrand
<Harald.T.Alvestrand@uninett.no>, has decided to try, and asks that if you
use Linux, you send a message to <linux-counter@uninett.no> with one of
the following subjects: `I use Linux at home', `I use Linux at work', or
`I use Linux at home and at work'.  He will also accept `third-party'
registrations - ask him for details.

He posts his counts to comp.os.linux.misc each month; alternatively look
on aun.uninett.no in /pub/misc/linux-counter.

- -----------------------------------------------------------------------------

Question 8.6.  How should I pronounce Linux ?

This is a matter of religious debate, of course !

If you want to hear the Linus himself say how he pronounces it download
english.au or swedish.au from ftp.funet.fi (in
/pub/OS/Linux/PEOPLE/Linus/SillySounds).  If you have a soundcard or the
PC-speaker audio driver you can hear them by typing
   cat english.au >/dev/audio
The difference isn't in the pronunciation of Linux but in the language
Linus uses to say hello.  The English version was parodied very well by
Jin Choi as "Hi, my name is Leenoos Torvahlds and I pronounce Leenooks as
Leenooks."

For the benefit of those of you who don't have the equipment or
inclination: Linus pronounces Linux approximately as Leenus, where the ee
is as in feet but rather shorter and the u is like a much shorter version
of the French eu sound in peur (pronouncing it as the u in put is probably
passable).

When speaking English I pronounce it Lie-nucks (u as in bucket) --- this
is an anglicised pronunciation based on the analogy with Linus' name,
which in English is usually pronounced Lie-nus (u as in put).  It is of
course quite acceptable and common to modify the pronunciation of a proper
noun when it changes languages.

I think I can safely say that the pronunciation Linnucks (short i as in
pit, short u as in bucket) is wrong in English, as it is not the original
Swedish pronunciation, not a sensible direct anglicisation of it, and not
based on the anglicised version of Linus' name.

===============================================================================

Section 9.  Frequently encountered error messages

 Q9.1        During linking I get Undefined symbol _mcount
 Q9.2        lp1 on fire
 Q9.3        INET: Warning: old style ioctl(IP_SET_DEV) called!
 Q9.4        ld: unrecognized option '-m486'
 Q9.5        GCC says Internal compiler error
 Q9.6        make says Error 139
 Q9.7        shell-init: permission denied when I log in.
 Q9.8        No utmp entry.  You must exec ... when I log in.
 Q9.9        Warning - bdflush not running
 Q9.10       Warning: obsolete routing request made.
 Q9.11       EXT2-fs: warning: mounting unchecked filesystem
 Q9.12       EXT2-fs warning: maximal count reached
 Q9.13       EXT2-fs warning: checktime reached
 Q9.14       df says Cannot read table of mounted filesystems
 Q9.15       fdisk says Partition X has different physical/logical ...
 Q9.16       fdisk: Partition 1 does not start on cylinder boundary
 Q9.17       fdisk says partition n has an odd number of sectors
 Q9.18       mtools says cannot initialise drive XYZ
 Q9.19       At the start of booting: Memory tight

- -----------------------------------------------------------------------------

Question 9.1.  During linking I get Undefined symbol _mcount

This is usually due to a bad interaction between a brokenness in SLS and
the C library release notes.  Your libc.a has been replaced by the
profiling library.  You should remove libc.a, libg.a and libc_p.a and once
again install the new libraries (following the release notes, of course).

- -----------------------------------------------------------------------------

Question 9.2.  lp1 on fire

This is a joke/traditional error message indicating that some sort of
error is being reported by your printer, but that the error status isn't a
valid one.  It may be that you have some kind of I/O or IRQ conflict -
check your cards' settings.  Some people report that they get this message
when their printer is switched off.  Hopefully it isn't really on fire ...

In newer kernels this message reads lp1 reported invalid error status (on
fire, eh?).

- -----------------------------------------------------------------------------

Question 9.3.  INET: Warning: old style ioctl(IP_SET_DEV) called!

You are trying to use the old network configuration utilities; the new
ones can be found on tsx-11.mit.edu in
/pub/linux/packages/net/net-2/binaries.

Note that they cannot be used just like the old-style programs; see the
NET-2 HOWTO for instructions on how to set up networking correctly.

- -----------------------------------------------------------------------------

Question 9.4.  ld: unrecognized option '-m486'

You have an old version of ld.  Install a newer binutils package -- this
will contain an updated ld.  Look on tsx-11.mit.edu in
/pub/linux/packages/GCC for binutils.tar.z.

- -----------------------------------------------------------------------------

Question 9.5.  GCC says Internal compiler error

If the fault is repeatable (ie, it always happens at the same place in the
same file --- even after rebooting and trying again, using a stable
kernel) you have discovered a bug in GCC.  See the GCC Info documentation
(type Control-h i in Emacs, and select GCC from the menu) for details on
how to report this -- make sure you have the latest version though.

Note that this is probably not a Linux-specific problem; unless you were
compiling a program many other Linux users also compile you should not
post your bug report to any of the comp.os.linux groups.

If the problem is not repeatable you are very probably experiencing memory
corruption --- see Q9.6 `make says Error 139'.

- -----------------------------------------------------------------------------

Question 9.6.  make says Error 139

Your compiler driver (gcc) dumped core.  You probably have a corrupted,
buggy or old version of GCC --- get the latest release.  Alternatively you
may be running out of swap space --- see Q6.6 `My machine runs very slowly
when I run GCC / X / ...' for more info.

If this doesn't fix the problem you are probably having problems with
memory or disk corruption.  Check that the clock rate, wait states and
refresh timing for your SIMMs are correct.  If so you may have some dodgy
SIMMs or a faulty motherboard or hard disk or controller.

Linux, like any Unix, is a very good memory tester --- much better than
DOS-based memory test programs.

Reportedly some clone x87 maths coprocessors can cause problems; try
compiling a kernel with maths emulation [Q7.6 `How do I upgrade/recompile
my kernel ?']; you may need to use the no387 kernel command line flag on
the LILO prompt to force the kernel to use it, or it may be able to work
and still use the 387, with the maths emulation compiled in but mainly
unused.

- -----------------------------------------------------------------------------

Question 9.7.  shell-init: permission denied when I log in.

Your root directory and all the directories up to your home directory must
be readable and executable by everybody.  See the manpage for chmod or a
book on Unix for how to fix the problem.

- -----------------------------------------------------------------------------

Question 9.8.  No utmp entry.  You must exec ... when I log in.

Your /var/adm/utmp is screwed up.  You should have
   > /var/adm/utmp
in your /etc/rc or /etc/rc.local.  See Q6.9 `I have screwed up my system
and can't log in to fix it.' for how to be able to do this.

- -----------------------------------------------------------------------------

Question 9.9.  Warning - bdflush not running

The development kernel series now uses a better strategy for writing
cached disk blocks.  In addition to the kernel changes, this involves
replacing the old update program which used to write everything every 30
seconds with a more subtle daemon (actually a pair), known as bdflush.

Get bdflush-n.n.tar.gz from the same place as the kernel source code [Q7.6
`How do I upgrade/recompile my kernel ?'] and compile and install it; it
should be started before the usual boot-time filesystem checks.  It will
work fine with older kernels as well, so there's no need to keep the old
update around.

- -----------------------------------------------------------------------------

Question 9.10.  Warning: obsolete routing request made.

This is nothing to worry about; it just means that the version of route
you have is a little out of date compared to the kernel.  You can make the
message go away by getting a new version of route from the same place as
the kernel source code [Q7.6 `How do I upgrade/recompile my kernel ?'].

- -----------------------------------------------------------------------------

Question 9.11.  EXT2-fs: warning: mounting unchecked filesystem

You need to run e2fsck (or fsck -t ext2 if you have the fsck front-end
program) with the -a option to get it to clear the `dirty' flag, and then
cleanly unmount the partition during each shutdown.

The easiest way to do this is to get the latest fsck, umount and shutdown
commands, available in Rik Faith's util-linux package [Q2.5 `Where can I
get Linux material by FTP ?'].  You have to make sure that your /etc/rc
scripts use them correctly.

NB don't try to check a filesystem that's mounted read-write - this
includes the root partition if you don't see
   VFS: mounted root ... read-only
at boot time.  You must arrange for to initially mount the root filesystem
readonly, check it if necessary, and then remount it read-write.  Read the
documentation that comes with util-linux to find out how to do this.

Note that you need to specify the -n option to mount to get it not to try
to update /etc/mtab, since the root filesystem is still read-only and this
will otherwise cause it to fail !

- -----------------------------------------------------------------------------

Question 9.12.  EXT2-fs warning: maximal count reached

This message is issued by the kernel when it mounts a filesystem that's
marked as clean, but whose `number of mounts since check' counter has
reached the predifined value.  The solution is to get the latest version
of the ext2fs utilities (e2fsprogs-0.5a.tar.gz at the time of writing)
from the usual sites [Q2.5 `Where can I get Linux material by FTP ?'].

The maximal number of mounts value can be examined and changed using the
tune2fs program from this package.

- -----------------------------------------------------------------------------

Question 9.13.  EXT2-fs warning: checktime reached

Kernels from 1.0 onwards support checking a filesystem based on the
elapsed time since the last check as well as by the number of mounts.  Get
the latest version of the ext2fs utilities [see Q9.12 `EXT2-fs warning:
maximal count reached'].

- -----------------------------------------------------------------------------

Question 9.14.  df says Cannot read table of mounted filesystems

There is probably something wrong with your /etc/mtab or /etc/fstab files.
If you have a reasonably new version of mount, /etc/mtab should be emptied
or deleted at boot time (in /etc/rc or /etc/rc.local), using something
like
   rm -f /etc/mtab*

Some versions of SLS have an entry for the root partition in /etc/mtab
made in /etc/rc by using rdev.  This is incorrect -- the newer versions of
mount do this automatically.

Other versions of SLS have a line in /etc/fstab that looks like:
    /dev/sdb1   /root   ext2   defaults
This is wrong.  /root should read simply /.

- -----------------------------------------------------------------------------

Question 9.15.  fdisk says Partition X has different physical/logical ...

If the partition number (X, above) is 1 this is the same problem as Q9.16
`fdisk: Partition 1 does not start on cylinder boundary'.

If the partition begins or ends on a cylinder numbered beyond 1024, this
is because standard DOS disk geometry information format in the partition
table can't cope with cylinder numbers with more than 10 bits.

This will cause DOS to be unable to access the partition correctly, and
will make booting a Linux kernel from that partition using LILO
problematic at best.

You can still use the partition for Linux or other operating systems that
use linear addressing (ie, number the disk blocks sequentially without
looking at heads, tracks and sectors).

I'd recommend creating at least one Linux partition entirely under the
1024-cylinder limit and booting off that; the other partitions will then
be OK.

- -----------------------------------------------------------------------------

Question 9.16.  fdisk: Partition 1 does not start on cylinder boundary

The version of fdisk that comes with many Linux systems creates partitions
that fail its own validity checking.  Unfortunately if you've already
installed your system there's not much you can do about this, apart from
copying the data off the partition, deleting and remaking it, and copying
the data back.

You can avoid the problem by getting the latest version of fdisk, from Rik
Faith's util-linux package (available on all good FTP sites).
Alternatively, if you are creating a new partition 1 that starts in the
first cylinder, you can do the following to get a partition that fdisk
likes.

1. Create partition 1 in the normal way.  A p listing will produce the
mismatch complaint.

2. Type u to set sector mode and do p again.  Copy down the number from
the "End" column.

3. Delete partition 1.

4. While still in sector mode recreate partition 1.  Set the first sector
to match the number of sectors per track.  This is the sector number in
the first line of the p output.  Set the last sector to the value noted in
2. above.

5. Type u to reset cylinder mode and continue with other partitions.

Ignore the message about unallocated sectors - they refer to the sectors
on the first track apart from the Master Boot Record, which are not used
if you start the first partition in track 2.

- -----------------------------------------------------------------------------

Question 9.17.  fdisk says partition n has an odd number of sectors

The PC disk partitioning scheme works in 512-byte sectors, but Linux uses
1K blocks.  If you have a partition with an odd number of sectors the last
sector is wasted.  Ignore the message.

- -----------------------------------------------------------------------------

Question 9.18.  mtools says cannot initialise drive XYZ

This means that mtools is having trouble accessing the drive.  This can be
due to several things.

Often this is due to the permissions on floppy drive devices (/dev/fd0*
and /dev/fd1*) being incorrect --- the user running mtools must have the
appropriate access.  See the manpage for chmod for details.

Most versions of mtools distributed with Linux systems (not the standard
GNU version) use the contents of a file /etc/mtools to discover which
devices and densities to use, in place of having this information compiled
into the binary.  Mistakes in this file often cause problems.  There is
often no documentation about this --- distribution packagers please note
that this is *evil*.

For the easiest way to access your DOS files (especially those on a hard
disk partition) see Q3.2 `How do I access files on my DOS partition or
floppy ?'.  Note - you should never use mtools to access files on an
msdosfs mounted partition or disk !

- -----------------------------------------------------------------------------

Question 9.19.  At the start of booting: Memory tight

This means that you have an extra large kernel that means that Linux has
to do some special memory-management magic to be able to boot itself from
the BIOS.  It isn't related to the amount of physical memory in your
machine.  Ignore the message, or compile a kernel containing only the
drivers and features you need [Q7.6 `How do I upgrade/recompile my kernel
?'].

===============================================================================

Section 10.  The X Window System

 Q10.1       Does Linux support X Windows ?
 Q10.2       Where can I get an XF86Config for my system ?
 Q10.3       xterm logins show up strangely in who, finger
 Q10.4       I can't get X Windows to work right.

- -----------------------------------------------------------------------------

Question 10.1.  Does Linux support X Windows ?

Yes.  Linux uses XFree86 (the current version is 3.1, which is based on
X11R6).  You need to have a video card which is supported by XFree86.  See
the Linux XFree86 HOWTO for more details.

Some of the Linux releases -- MCC, for example -- don't come with X
Windows already included; however you can easily download and install it
from /pub/Linux/X11/Xfree86-* on sunsite.unc.edu and its mirror sites.
Read the XFree86 HOWTO for installation instructions.

Other releases -- Slackware, Debian, TAMU and SLS, for example -- come
with X Windows already included

- -----------------------------------------------------------------------------

Question 10.2.  Where can I get an XF86Config for my system ?

See the Linux XFree86 HOWTO.

You'll need to put together your own XF86Config file, because it depends
on the exact combination of video card and monitor you have.  It's not
that hard to do -- read the instructions that came with XFree86, in
/usr/X11R6/lib/X11/etc.  The file you probably most need to look at is
README.Config.

For a quick start you may run the program xf86config.  Note that
ConfigXF86 is now obsolete and you shouldn't use it.

Please don't post to comp.os.linux.help asking for an XF86Config.

- -----------------------------------------------------------------------------

Question 10.3.  xterm logins show up strangely in who, finger

The xterm that comes with XFree86 2.1 and earlier doesn't correctly
understand the format that Linux uses for the /var/adm/utmp file, where
the system records who is logged in.  It therefore doesn't set all the
information correctly.

XFree86 3.1 fixes this problem.

- -----------------------------------------------------------------------------

Question 10.4.  I can't get X Windows to work right.

Read the XFree86 HOWTO - note the question and answer section.

Try reading comp.windows.x.i386unix -- specifically read the the FAQ for
that group.

Please don't post X Windows or XFree86 related questions to
comp.os.linux.help unless they are Linux-specific.

===============================================================================

Section 11.  Questions applicable to very out-of-date software

 Q11.1       fdisk says cannot use nnn sectors of this partition
 Q11.2       GCC sometimes uses huge amounts of virtual memory and thrashes
 Q11.3       My keyboard goes all funny after I switch VC's.

The questions in this section are only relevant to users of software that
is at least 3 months old.

Please let me know if you find the answer to a problem you had here, as
unused questions in this section will eventually disappear [Q13.1
`Feedback is invited'].

- -----------------------------------------------------------------------------

Question 11.1.  fdisk says cannot use nnn sectors of this partition

Originally Linux only supported the Minix filesystem, which cannot use
more than 64Mb per parition.  This limitation is not present in the more
advanced filesystems now available, such as ext2fs (the 2nd version of the
Extended Filesystem) and xiafs (Qi Xia's filesystem).

If you intend to use ext2fs or xiafs you can ignore the message.

- -----------------------------------------------------------------------------

Question 11.2.  GCC sometimes uses huge amounts of virtual memory and thrashes

Older versions of GCC had a bug which made them use lots of memory if you
tried to compile a program which had a large static data table in it.

You can either upgrade your version of GCC to at least version 2.5, or add
more swap if necessary and just grin and bear it; it'll work in the end.

- -----------------------------------------------------------------------------

Question 11.3.  My keyboard goes all funny after I switch VC's.

This is a bug in kernel versions before 0.99pl14-alpha-n.  Sometimes Linux
loses track of what modifier keys (Shift, Alt, Control etc.) are pressed
or not, and believes that one or more are pressed when they are not.  The
solution is to press and release each of the modifier keys (without
pressing any other keys) --- this will ensure that Linux knows what state
the keyboard is actually in.

This problem often occurs when switching out of X windows; it can
sometimes be avoided by releasing Ctrl and Alt very quickly after pressing
the F-key of the VC you are switching to.

===============================================================================

Section 12.  How to get further assistance

 Q12.1       You still haven't answered my question !
 Q12.2       What to put in a posting to comp.os.linux.help
 Q12.3       I want to mail someone about my problem.

- -----------------------------------------------------------------------------

Question 12.1.  You still haven't answered my question !

Please read all of this answer before posting.  I know it's a bit long,
but you may be about to make a fool of yourself in front of 50000 people
and waste hundreds of hours of their time.  Don't you think it's worth it
to spend some of your time reading and following these instructions ?

If you think an answer is incomplete or inaccurate, please mail Ian
Jackson at <ijackson@nyx.cs.du.edu>.

Read the appropriate Linux Documentation Project books - see Q2.1 `Where
can I get the HOWTOs and other documentation ?'.

If you're a Unix newbie read the FAQ for comp.unix.questions, and those
for any of the other comp.unix.* groups that may be relevant.

Linux is a Unix clone, so almost everything you read there will apply to
Linux.  Those FAQs can, like all FAQs, be found on rtfm.mit.edu in
/pub/usenet/news.answers (the mail-server@rtfm.mit.edu can send you these
files, for those who don't have FTP access).  There are mirrors of rtfm's
FAQ artchives on various sites - check the Introduction to *.answers
posting, posted, or look in news-answers/introduction in the directory
above.

Check the relevant HOWTO for the subject in question, if there is one, or
an appropriate old-style sub-FAQ document.  Check the FTP sites.

Try experimenting --- that's the best way to get to know Unix and Linux.

Read the documentation.  Check the manpages (type man man if you don't
know about manpages.  Try man -k <subject> --- it often lists useful and
relevant manpages.

Check the Info documentation (type C-h i, i.e. Control H followed by I in
Emacs) --- NB this isn't just for Emacs; for example the GCC documentation
lives here as well.

There will also often be a README file with a package giving installation
and/or usage instructions.

Make sure that you don't have a corrupted or out-of-date copy of the
program in question.  If possible, download it again and reinstall it ---
perhaps you made a mistake the first time.

Read comp.os.linux.announce --- this often contains very important
information for all Linux users.

X-Windows questions belong in comp.windows.x.i386unix, not in
comp.os.linux.help.  But read the group first (including the FAQ), before
you post !

Only if you have done all of these things and are still stuck should you
post to comp.os.linux.help.  Make sure you read the next question, Q12.2
`What to put in a posting to comp.os.linux.help', first.

- -----------------------------------------------------------------------------

Question 12.2.  What to put in a posting to comp.os.linux.help

Please read carefully the following advice about how to write your
posting.  Taking heed of it will greatly increase the chances that an
expert and/or fellow user reading your posting will have enough
information and motivation to reply.

Make sure you give full details of the problem, including:

* What program, exactly, you are having problems with.  Include the
  version number if known and say where you got it.  Many standard
  commands tell you their version number if you give them a --version
  option.

* Which Linux release you're using (MCC, Slackware, Debian or whatever)
  and what version of that release.

* The *exact* and *complete* text of any error messages printed.

* Exactly what behaviour you were expecting, and exactly what behaviour
  you observed.  A transcript of an example session is a good way of
  showing this.

* The contents of any configuration files used by the program in question
  and any related programs.

* What version of the kernel and of the shared libraries you are using.
  The kernel version can be found by typing uname -a, and the shared
  library version by typing ls -l /lib/libc.so.4.

* Details of what hardware you're running on, if it seems appropriate.

You are in little danger of making your posting too long unless you
include large chunks of source code or uuencoded files, so err on the side
of giving too much information.

Use a clear, detailed Subject line.  Don't put things like `doesn't work',
`Linux', `help' or `question' in it --- we already knew that ! Save the
space for the name of the program, a fragment of the error message,
summary of the unusual behaviour, etc.

If you are reporting an `unable to handle kernel paging request' message,
follow the instructions in the Linux kernel sources README for turning the
numbers into something more meaningful.  If you don't do this noone who
reads your post will be able to do it for you, as the mapping from numbers
to function names varies from one kernel to another.

Put a summary paragraph at the top of your posting.

At the bottom of your posting, ask for responses by email and say you'll
post a summary.  Back this up by using Followup-To: poster.  Then, do
actually post a summary in a few days or a week or so.  Don't just
concatenate the replies you got --- summarise.  Putting the word SUMMARY
in your summary's Subject line is also a good idea.  Consider submitting
the summary to comp.os.linux.announce.

Make sure your posting doesn't have an inappropriate References header
line.  This marks your article as part of the thread of the article
referred to, which will often cause it to be junked by the readers with
the rest of a boring thread.

You might like to say in your posting that you've read this FAQ and the
appropriate HOWTOs - this may make people less likely to skip your
posting.

Remember that you should not post email sent to you personally without the
sender's permission.

- -----------------------------------------------------------------------------

Question 12.3.  I want to mail someone about my problem.

Try to find the author or developer of whatever program or component is
causing you difficulty.  If you have a contact point for the Linux
distribution you are using you should use it.

Please put everything in your email that you would put in a posting asking
for help.

Finally, remember that despite the fact that most of the Linux community
are very helpful and responsive to emailed questions you'll be asking for
help from an unpaid volunteer, so you have no right to expect an answer.

===============================================================================

Section 13.  Administrative information and acknowledgements

 Q13.1       Feedback is invited
 Q13.2       Formats in which this FAQ is available
 Q13.3       Authorship and acknowledgements
 Q13.4       Disclaimer and Copyright

- -----------------------------------------------------------------------------

Question 13.1.  Feedback is invited

Please send me your comments on this FAQ.

I accept submissions for the FAQ in any format;  All contributions
comments and corrections are gratefully received.

Please send them to <ijackson@nyx.cs.du.edu>.

By the way, if you wish to refer to a question(s) in the FAQ it's most
useful for me if you do so by the question heading, rather than the
number, as the question numbers are generated automatically and I don't
see them in the source file I edit.

- -----------------------------------------------------------------------------

Question 13.2.  Formats in which this FAQ is available

This document is available as an ASCII text file, an Emacs Info document,
an HTML World Wide Web page, PostScript and as a USENET news posting.

The ASCII, Emacs Info, HTML and posted versions and a Lout typesetter file
(from which the PostScript is produced) are generated automatically by a
Perl script which takes as input a file in the Bizarre Format with No
Name.

The output files linux-faq.ascii, .info and .ps and a tarfile
linux-faq.source.tar.gz, containing the BFNN source and Perl script
converter, are available in the docs directories of the major Linux FTP
sites.

The HTML version of this FAQ is available as
http://www.cl.cam.ac.uk/users/iwj10/linux-faq/index.html.

The USENET version is posted regularly to comp.os.linux.announce,
comp.os.linux.help, comp.answers and news.answers.

- -----------------------------------------------------------------------------

Question 13.3.  Authorship and acknowledgements

This FAQ was compiled by Ian Jackson <ijackson@nyx.cs.du.edu>, with
assistance and comments from others too numerous to mention.  It was
loosely based on the original Linux FAQ by Marc-Michel Corsini.

Special thanks are due to Matt Welsh, who coordinates the HOWTOs and has
written substantial portions of many of them, and to Marc-Michel Corsini.
Thanks also to the contributors to the previous Linux FAQ, and to those
sent me comments about this FAQ, and who answered questions on the
newsgroup.

Last but not least, thanks to Linus Torvalds and the other contributors to
Linux for giving us something to write about !

- -----------------------------------------------------------------------------

Question 13.4.  Disclaimer and Copyright

Note that this document is provided as is.  The information in it is *not*
warranted to be correct; you use it at your own risk.

Linux Frequently Asked Questions with Answers is Copyright 1994 by Ian
Jackson <ijackson@nyx.cs.du.edu>.

It may be reproduced and distributed in its entirity (including this
authorship, copyright and permission notice) provided that either:

* the distribution is not commercial (commercial means any situation in
  which you benefit financially - directly or indirectly such as by
  inclusion in a publication which carries commercial advertising), or
* the distribution is in machine-readable form (ie, a form intended to be
  easily processed by a computer).

Note that this restriction is not intended to prohibit charging for the
service of printing or copying a document supplied by your customer.

Any distribution of a partial copy or extract, a translation or a
derivative work must be approved by me before distribution.  Email me -
I'll probably be happy to oblige !

Exceptions to these rules may be granted, and I shall be happy to answer
any questions about this copyright --- write to Ian Jackson, Churchill
College, Cambridge, CB3 0DS, United Kingdom or email
<ijackson@nyx.cs.du.edu>.  These restrictions are here to protect the
contributors, not to restrict you as educators and learners.

Ian Jackson asserts the right to be identified as the author of this work,
and claims the moral rights of paternity and integrity, in accordance with
the Copyright, Designs and Patents Act, 1988.


-----BEGIN PGP SIGNATURE-----
Version: 2.6

iQCVAgUBLy7NdsMWjroj9a3bAQHmGQP/RakVY+TRrcr25Bf5XzsBsrV7TywmHUJa
HKoEUZIOGiuOnKpgicauaVnUw7CnrNMOjrKRO9GVnagiyM2TelJtnQWdA07Rvrcc
fWuGk7Huh3p7oXsXtlxLGvqcmr0JzoaGFEmtjBMAvBA+mxPiv/zTwxu2jaUtkPLy
iiCWIbT8oTI=
=wDu/
-----END PGP SIGNATURE-----
-- 
Ian Jackson, at home.         ijackson@nyx.cs.du.edu or iwj10@cus.cam.ac.uk
+44 1223 575512    Escoerea on IRC.   http://www.cl.cam.ac.uk/users/iwj10/
2 Lexington Close, Cambridge, CB4 3LS, England.   Urgent: iwj@cam-orl.co.uk

